Connect Keithly to computer using GPIB

Type the following into the command prompt/terminal:

ipython

from PLQY import PJV

cd /into your directory/

p = PJV.pJV()

p.take\_pJV(sample\_name = "sample", min\_current = 300, max\_current = 800, step = 20, n\_wires = 2)

# change sample name, modify min and max current as needed